{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["MENU","一覧","DATATBL","▼拾い集計"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":1},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MENU","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"一覧","index":1,"n_rows":15,"n_cols":17,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["区分1","配管"]
[]
["合計 / 数量",null,"サイズ"]
["名称1","名称2","100A","12.7φ×6.4φ","15.9φ×9.5φ","15A","19.1φ×9.5φ","20A","20Su","25A","25Su","32A","34.9φ×9.5φ","40A","50A","65A","80A"]
["ドレン(空調)","配管用炭素鋼鋼管(白)",null,null,null,null,null,313,null,29993,null,49087,null,42983,117]
["汚水","硬質塩化ビニル管(VP)",null,null,null,null,null,null,null,null,null,null,null,null,118]
[null,"排水用硬質塩化ビニルライニング鋼管",44146,null,null,null,null,null,null,null,null,null,null,20497,39055,4675,6419]
["屋内消火栓","配管用炭素鋼鋼管(白)",null,null,null,null,null,null,null,null,null,null,null,9536,4493,39444]
["給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)",null,null,null,183,null,47701,null,13789,null,5860,null,1641,10643,1950]
["給湯(往)","一般配管用ステンレス鋼管",null,null,null,null,null,null,26174,null,51050]
["給湯(還)","一般配管用ステンレス鋼管",null,null,null,null,null,null,44116,null,700]
["通気","排水用硬質塩化ビニルライニング鋼管",null,null,null,null,null,null,null,null,null,null,null,null,null,6633,11131]
[null,"配管用炭素鋼鋼管(白)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,21424]
["冷媒","冷媒用銅管(2管式)",null,56678,16744,null,7018,null,null,null,null,null,19337]
["総計",null,44146,56678,16744,183,7018,48014,70290,43782,51750,54947,19337,74657,54426,52702,38974]

{"sheet":"DATATBL","index":2,"n_rows":339,"n_cols":10,"rows_kept":339,"cut":false,"hidden":false,"merged":[]}
["区分1","名称1","名称2","名称3","名称4","名称5","サイズ","数量","単位","備考"]
["配管","冷媒","冷媒用銅管(2管式)","-","-","-","12.7φ×6.4φ",56678,"mm","-"]
["配管","冷媒","冷媒用銅管(2管式)","-","-","-","15.9φ×9.5φ",16744,"mm","-"]
["配管","冷媒","冷媒用銅管(2管式)","-","-","-","19.1φ×9.5φ",7018,"mm","-"]
["配管","冷媒","冷媒用銅管(2管式)","-","-","-","34.9φ×9.5φ",19337,"mm","-"]
["配管","ドレン(空調)","配管用炭素鋼鋼管(白)","-","-","-","20A",313,"mm","-"]
["配管","ドレン(空調)","配管用炭素鋼鋼管(白)","-","-","-","25A",29993,"mm","-"]
["配管","ドレン(空調)","配管用炭素鋼鋼管(白)","-","-","-","32A",49087,"mm","-"]
["配管","ドレン(空調)","配管用炭素鋼鋼管(白)","-","-","-","40A",42983,"mm","-"]
["配管","ドレン(空調)","配管用炭素鋼鋼管(白)","-","-","-","50A",117,"mm","-"]
["配管","給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)","-","-","-","15A",183,"mm","-"]
["配管","給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)","-","-","-","20A",47701,"mm","-"]
["配管","給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)","-","-","-","25A",13789,"mm","-"]
["配管","給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)","-","-","-","32A",5860,"mm","-"]
["配管","給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)","-","-","-","40A",1641,"mm","-"]
["配管","給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)","-","-","-","50A",10643,"mm","-"]
["配管","給水","水道用硬質塩化ビニルライニング鋼管(屋内外用)","-","-","-","65A",1950,"mm","-"]
["配管","給湯(往)","一般配管用ステンレス鋼管","-","-","-","20Su",26174,"mm","-"]
["配管","給湯(往)","一般配管用ステンレス鋼管","-","-","-","25Su",51050,"mm","-"]
["配管","給湯(還)","一般配管用ステンレス鋼管","-","-","-","20Su",44116,"mm","-"]
["配管","給湯(還)","一般配管用ステンレス鋼管","-","-","-","25Su",700,"mm","-"]
["配管","汚水","排水用硬質塩化ビニルライニング鋼管","-","-","-","40A",20497,"mm","-"]
["配管","汚水","排水用硬質塩化ビニルライニング鋼管","-","-","-","50A",39055,"mm","-"]
["配管","汚水","排水用硬質塩化ビニルライニング鋼管","-","-","-","65A",4675,"mm","-"]
["配管","汚水","排水用硬質塩化ビニルライニング鋼管","-","-","-","80A",6419,"mm","-"]
["配管","汚水","排水用硬質塩化ビニルライニング鋼管","-","-","-","100A",44146,"mm","-"]
["配管","汚水","硬質塩化ビニル管(VP)","-","-","-","50A",118,"mm","-"]
["配管","通気","排水用硬質塩化ビニルライニング鋼管","-","-","-","65A",6633,"mm","-"]
["配管","通気","排水用硬質塩化ビニルライニング鋼管","-","-","-","80A",11131,"mm","-"]
["配管","通気","配管用炭素鋼鋼管(白)","-","-","-","80A",21424,"mm","-"]
["配管","屋内消火栓","配管用炭素鋼鋼管(白)","-","-","-","40A",9536,"mm","-"]
["配管","屋内消火栓","配管用炭素鋼鋼管(白)","-","-","-","50A",4493,"mm","-"]
["配管","屋内消火栓","配管用炭素鋼鋼管(白)","-","-","-","65A",39444,"mm","-"]
["継手","冷媒","セパレータ","-","-","-","15.9φ(9.5φ)×12.7φ(6.4φ)×12.7φ(6.4φ)",1,"個","-"]
["継手","冷媒","セパレータ","-","-","-","15.9φ(9.5φ)×15.9φ(9.5φ)×12.7φ(6.4φ)",1,"個","-"]
["継手","冷媒","セパレータ","-","-","-","19.1φ(9.5φ)×15.9φ(9.5φ)×12.7φ(6.4φ)",1,"個","-"]
["継手","冷媒","セパレータ","-","-","-","19.1φ(9.5φ)×19.1φ(9.5φ)×12.7φ(6.4φ)",1,"個","-"]
["継手","冷媒","セパレータ","-","-","-","34.9φ(9.5φ)×12.7φ(6.4φ)×12.7φ(6.4φ)",1,"個","-"]
["継手","冷媒","セパレータ","-","-","-","34.9φ(9.5φ)×34.9φ(9.5φ)×12.7φ(6.4φ)",2,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","L","-","-","40",3,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","L","-","-","50×40",1,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","P","-","-","32",1,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","S","-","-","40×32",1,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","S","-","-","50×32",1,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","S","-","-","50×40",1,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","ST","-","-","32",13,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","ST","-","-","40×32",1,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","TY","-","-","40",3,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","TY","-","-","40×32",3,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","YL","-","-","32",9,"個","-"]
["継手","ドレン(空調)","ドレネジ継手","YL","-","-","40",3,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","L","-","-","25",29,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","P","-","-","25",15,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","P","-","-","32",7,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","P","-","-","40",3,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","S","-","-","25",2,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","S","-","-","25×20",1,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","S","-","-","32×25",10,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","T","-","-","25",14,"個","-"]
["継手","ドレン(空調)","鋼管継手（白）","YL","-","-","25",4,"個","-"]
["継手","給水","メーター接続金具","ガス管用U","-","-","25",3,"個","-"]
["継手","給水","屋内用管端防食継手","L","-","-","20",41,"個","-"]
["継手","給水","屋内用管端防食継手","L","-","-","25",11,"個","-"]
["継手","給水","屋内用管端防食継手","L","-","-","32",2,"個","-"]
["継手","給水","屋内用管端防食継手","L","-","-","40",1,"個","-"]
["継手","給水","屋内用管端防食継手","L","-","-","50",5,"個","-"]
["継手","給水","屋内用管端防食継手","L","-","-","20×15",1,"個","-"]
["継手","給水","屋内用管端防食継手","S","-","-","20×15",5,"個","-"]
["継手","給水","屋内用管端防食継手","S","-","-","25×20",4,"個","-"]
["継手","給水","屋内用管端防食継手","S","-","-","32×20",1,"個","-"]
["継手","給水","屋内用管端防食継手","S","-","-","32×25",1,"個","-"]
["継手","給水","屋内用管端防食継手","S","-","-","40×32",1,"個","-"]
["継手","給水","屋内用管端防食継手","S","-","-","50×32",1,"個","-"]
["継手","給水","屋内用管端防食継手","S","-","-","65×50",1,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","20",2,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","25",1,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","50",1,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","25×20",7,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","32×20",4,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","32×25",4,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","40×25",2,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","50×40",1,"個","-"]
["継手","給水","屋内用管端防食継手","T","-","-","65×50",1,"個","-"]
["継手","給水","屋内用管端防食継手","YL","-","-","50",1,"個","-"]
["継手","給水","屋内用管端防食継手","給水栓L","-","-","20",1,"個","-"]
["継手","給水","鋳鉄製フランジ","F10K","-","-","65",2,"個","-"]
["継手","給湯(往)","BKジョイント","L","-","-","20",16,"個","-"]
["継手","給湯(往)","BKジョイント","L","-","-","25",17,"個","-"]
["継手","給湯(往)","BKジョイント","S","-","-","25×20",4,"個","-"]
["継手","給湯(往)","BKジョイント","T","-","-","20",4,"個","-"]
["継手","給湯(往)","BKジョイント","T","-","-","25",5,"個","-"]
["継手","給湯(往)","BKジョイント","T","-","-","25×20",4,"個","-"]
["継手","給湯(往)","BKジョイント","YL","-","-","25",2,"個","-"]
["継手","給湯(往)","BKジョイント","水栓S","-","-","20×15",1,"個","-"]
["継手","給湯(往)","BKジョイント","雄アダプタ付S","-","-","20×20",1,"個","-"]
["継手","給湯(往)","BKジョイント","雄アダプタ付S","-","-","25×25",4,"個","-"]
["継手","給湯(還)","BKジョイント","L","-","-","20",21,"個","-"]
["継手","給湯(還)","BKジョイント","L","-","-","25",1,"個","-"]
["継手","給湯(還)","BKジョイント","S","-","-","20",1,"個","-"]
["継手","給湯(還)","BKジョイント","T","-","-","20",3,"個","-"]
["継手","給湯(還)","BKジョイント","T","-","-","25×20",1,"個","-"]
["継手","給湯(還)","BKジョイント","雄アダプタ付S","-","-","20×20",4,"個","-"]
["継手","給湯(還)","モルコジョイント","S","-","-","25×20",1,"個","-"]
["継手","汚水","MDジョイント","LL","-","-","40",12,"個","-"]
["継手","汚水","MDジョイント","LL","-","-","50",26,"個","-"]
["継手","汚水","MDジョイント","LL","-","-","65",4,"個","-"]
["継手","汚水","MDジョイント","LL","-","-","80",4,"個","-"]
["継手","汚水","MDジョイント","LL","-","-","100",8,"個","-"]
["継手","汚水","MDジョイント","S","-","-","100",1,"個","-"]
["継手","汚水","MDジョイント","ST","-","-","100×80",3,"個","-"]
["継手","汚水","MDジョイント","TY","-","-","50",2,"個","-"]
["継手","汚水","MDジョイント","TY","-","-","100",5,"個","-"]
["継手","汚水","MDジョイント","TY","-","-","100×40",4,"個","-"]
["継手","汚水","MDジョイント","TY","-","-","100×50",8,"個","-"]
["継手","汚水","MDジョイント","TY","-","-","100×65",3,"個","-"]
["継手","汚水","MDジョイント","TY","-","-","100×80",4,"個","-"]
["継手","汚水","MDジョイント","Y","-","-","100",2,"個","-"]
["継手","汚水","MDジョイント","Y","-","-","100×40",1,"個","-"]
["継手","汚水","MDジョイント","Y","-","-","100×50",3,"個","-"]
["継手","汚水","MDジョイント","YL","-","-","40",6,"個","-"]
["継手","汚水","MDジョイント","YL","-","-","50",2,"個","-"]
["継手","汚水","MDジョイント","YL","-","-","65",1,"個","-"]
["継手","汚水","MDジョイント","YL","-","-","80",5,"個","-"]
["継手","汚水","MDジョイント","YL","-","-","100",8,"個","-"]
["継手","汚水","MDジョイント","パッキンセット","-","-","40",41,"個","-"]
["継手","汚水","MDジョイント","パッキンセット","-","-","50",73,"個","-"]
["継手","汚水","MDジョイント","パッキンセット","-","-","65",13,"個","-"]
["継手","汚水","MDジョイント","パッキンセット","-","-","80",25,"個","-"]
["継手","汚水","MDジョイント","パッキンセット","-","-","100",109,"個","-"]
["継手","汚水","MDジョイント","満水試験用COS","-","-","100",2,"個","-"]
["継手","通気","MDジョイント","LL","-","-","65",2,"個","-"]
["継手","通気","MDジョイント","LL","-","-","80",13,"個","-"]
["継手","通気","MDジョイント","ST","-","-","80×65",2,"個","-"]
["継手","通気","MDジョイント","Y","-","-","80",1,"個","-"]
["継手","通気","MDジョイント","Y","-","-","80×65",1,"個","-"]
["継手","通気","MDジョイント","YL","-","-","65",3,"個","-"]
["継手","通気","MDジョイント","YL","-","-","80",4,"個","-"]
["継手","通気","MDジョイント","パッキンセット","-","-","65",13,"個","-"]
["継手","通気","MDジョイント","パッキンセット","-","-","80",43,"個","-"]
["継手","屋内消火栓","鋳鉄製フランジ","F10K","-","-","65",1,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","L","-","-","40",10,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","L","-","-","65",8,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","L","-","-","50×40",1,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","S","-","-","50",1,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","S","-","-","50×40",2,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","T","-","-","65",1,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","T","-","-","50×40×40",1,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","T","-","-","50×40×65",1,"個","-"]
["継手","屋内消火栓","鋼管継手（白）","T","-","-","50×50×65",1,"個","-"]
["弁類･特殊継手","給水","青銅製仕切弁(ねじ込み形)JIS10K","-","-","-","50",2,"個","-"]
["弁類･特殊継手","給湯(往)","自動空気抜き弁(ねじ込み形)","-","-","-","20",1,"個","-"]
["弁類･特殊継手","給湯(往)","青銅製仕切弁(ねじ込み形)JIS10K","-","-","-","20",1,"個","-"]
["弁類･特殊継手","給湯(往)","青銅製仕切弁(ねじ込み形)JIS10K","-","-","-","25",2,"個","-"]
["弁類･特殊継手","給湯(還)","青銅製仕切弁(ねじ込み形)JIS10K","-","-","-","20",2,"個","-"]
["弁類･特殊継手","汚水","COA 掃除口(ねじ込み形)","-","-","-","50",2,"個","-"]
["弁類･特殊継手","汚水","COA 掃除口(ねじ込み形)","-","-","-","100",1,"個","-"]
["弁類･特殊継手","汚水","COB 掃除口(防水用)","-","-","-","100",6,"個","-"]
["弁類･特殊継手","汚水","T3B 床排水トラップ(Pトラップ式)防水用","-","-","-","65",2,"個","-"]
["弁類･特殊継手","未設定の配管","サクションカバー(相フランジ形)","-","-","-","65",1,"個","-"]
["ダクト","給気","主管","アルミフレキ 100φ","-","-","400L",1,"本","-"]
["ダクト","給気","主管","アルミフレキ 100φ","-","-","440L",1,"本","-"]
["ダクト","給気","主管","アルミフレキ 100φ","-","-","550L",1,"本","-"]
["ダクト","給気","主管","アルミフレキ 100φ","-","-","650L",1,"本","-"]
["ダクト","給気","主管","アルミフレキ 100φ","-","-","760L",1,"本","-"]
["ダクト","給気","主管","アルミフレキ 150φ","-","-","550L",1,"本","-"]
["ダクト","給気","主管","ニューホープ 100φ","-","-","410L",1,"本","-"]
["ダクト","給気","スパイラルダクト","主管","亜鉛鉄板","-","100φ",19600.208999999999,"mm",0.5]
["ダクト","給気","スパイラルダクト","主管","亜鉛鉄板","-","150φ",11400.626,"mm",0.5]
["ダクト","外気","アングルフランジダクト","300×200","亜鉛鉄板","-","0.5mm",0.66,"㎡","-"]
["ダクト","外気","共板フランジダクト","300×200","亜鉛鉄板","-","0.5mm",5.8159999999999998,"㎡","-"]
["ダクト","外気","主管","ニューホープ 100φ","-","-","1670L",1,"本","-"]
["ダクト","外気","主管","ニューホープ 100φ","-","-","3470L",1,"本","-"]
["ダクト","外気","主管","ニューホープ 100φ","-","-","3570L",1,"本","-"]
["ダクト","外気","主管","ニューホープ 150φ","-","-","2270L",1,"本","-"]
["ダクト","外気","主管","ニューホープ 150φ","-","-","2320L",1,"本","-"]
["ダクト","外気","主管","ニューホープ 150φ","-","-","2460L",1,"本","-"]
["ダクト","外気","スパイラルダクト","主管","亜鉛鉄板","-","100φ",8561.1290000000008,"mm",0.5]
["ダクト","外気","スパイラルダクト","主管","亜鉛鉄板","-","150φ",1729.2639999999999,"mm",0.5]
["ダクト","外気","スパイラルダクト","主管","亜鉛鉄板","-","200φ",3532.7640000000001,"mm",0.5]
["ダクト","外気","スパイラルダクト","主管","亜鉛鉄板","-","250φ",14364.291999999999,"mm",0.5]
["ダクト","排気","共板フランジダクト","600×400","亜鉛鉄板","-","0.6mm",15.090999999999999,"㎡","-"]
["ダクト","排気","共板フランジダクト","700×670","亜鉛鉄板","-","0.6mm",1.548,"㎡","-"]
["ダクト","排気","円形フランジダクト","主管","亜鉛鉄板","-","750φ",375,"mm",0.8]
["ダクト","排気","主管","アルミフレキ 100φ","-","-","400L",1,"本","-"]
["ダクト","排気","主管","アルミフレキ 100φ","-","-","480L",1,"本","-"]
["ダクト","排気","主管","アルミフレキ 100φ","-","-","500L",1,"本","-"]
["ダクト","排気","主管","アルミフレキ 100φ","-","-","560L",1,"本","-"]
["ダクト","排気","主管","アルミフレキ 100φ","-","-","790L",1,"本","-"]
["ダクト","排気","主管","アルミフレキ 150φ","-","-","550L",1,"本","-"]
["ダクト","排気","主管","アルミフレキ 250φ","-","-","430L",1,"本","-"]
["ダクト","排気","主管","アルミフレキ 250φ","-","-","840L",1,"本","-"]
["ダクト","排気","主管","ニューホープ 100φ","-","-","400L",1,"本","-"]
["ダクト","排気","主管","ニューホープ 100φ","-","-","1660L",1,"本","-"]
["ダクト","排気","主管","ニューホープ 100φ","-","-","1940L",1,"本","-"]
["ダクト","排気","主管","ニューホープ 100φ","-","-","2150L",1,"本","-"]
["ダクト","排気","主管","ニューホープ 150φ","-","-","2130L",1,"本","-"]
["ダクト","排気","主管","ニューホープ 150φ","-","-","2350L",1,"本","-"]
["ダクト","排気","主管","ニューホープ 150φ","-","-","2620L",1,"本","-"]
["ダクト","排気","スパイラルダクト","主管","亜鉛鉄板","-","100φ",32937.086000000003,"mm",0.5]
["ダクト","排気","スパイラルダクト","主管","亜鉛鉄板","-","150φ",37720.432000000001,"mm",0.5]
["ダクト","排気","スパイラルダクト","主管","亜鉛鉄板","-","200φ",8883.7810000000009,"mm",0.5]
["ダクト","排気","スパイラルダクト","主管","亜鉛鉄板","-","250φ",14887.339,"mm",0.5]
["ダクト","未設定のダクト","スパイラルダクト","主管","亜鉛鉄板","-","150φ",50,"mm",0.5]
["ダクト","未設定のダクト","スパイラルダクト","主管","亜鉛鉄板","-","200φ",150.94300000000001,"mm",0.5]
["ダクト","未設定のダクト","スパイラルダクト","主管","亜鉛鉄板","-","250φ",50,"mm",0.5]
["ダクト器具","給気","FD","-","-","-","100φ×200L",1,"個","-"]
["ダクト器具","給気","FD","-","-","-","100φ×300L",1,"個","-"]
["ダクト器具","給気","キャンバス継手","-","-","-","100φ×200L",1,"個","-"]
["ダクト器具","給気","キャンバス継手","-","-","-","150φ×200L",4,"個","-"]
["ダクト器具","外気","ボックス(内貼り 25mm)","-","-","-","550×550×400H",2,"個","-"]
["ダクト器具","外気","FD","-","-","-","100φ×300L",1,"個","-"]
["ダクト器具","外気","FD","-","-","-","300×200×200L",1,"個","-"]
["ダクト器具","外気","キャンバス継手","-","-","-","100φ×200L",1,"個","-"]
["ダクト器具","外気","キャンバス継手","-","-","-","200φ×200L",1,"個","-"]
["ダクト器具","外気","ベントキャップ","-","-","-","VC 100φ",4,"個","-"]
["ダクト器具","外気","ベントキャップ","-","-","-","VC 150φ",3,"個","-"]
["ダクト器具","外気","ベントキャップ","-","-","-","VC 200φ",1,"個","-"]
["ダクト器具","外気","ベントキャップ","-","-","-","VC 250φ",2,"個","-"]
["ダクト器具","外気","レジスター","-","-","-","VHS 350×350",2,"個","-"]
["ダクト器具","外気","短管","-","-","-","350×350×150L",2,"個","-"]
["ダクト器具","排気","ボックス(内貼り 25mm)","-","-","-","400×450×400H",2,"個","-"]
["ダクト器具","排気","FD","-","-","-","100φ×200L",1,"個","-"]
["ダクト器具","排気","FD","-","-","-","100φ×300L",2,"個","-"]
["ダクト器具","排気","FD","-","-","-","150φ×200L",1,"個","-"]
["ダクト器具","排気","FD","-","-","-","150φ×300L",2,"個","-"]
["ダクト器具","排気","FD","-","-","-","200φ×300L",1,"個","-"]
["ダクト器具","排気","FD","-","-","-","250φ×200L",1,"個","-"]
["ダクト器具","排気","キャンバス継手","-","-","-","100φ×200L",2,"個","-"]
["ダクト器具","排気","キャンバス継手","-","-","-","150φ×200L",8,"個","-"]
["ダクト器具","排気","キャンバス継手","-","-","-","200φ×200L",3,"個","-"]
["ダクト器具","排気","キャンバス継手","-","-","-","250φ×200L",1,"個","-"]
["ダクト器具","排気","キャンバス継手","-","-","-","600×400(500φ)×362L",1,"個","-"]
["ダクト器具","排気","ベントキャップ","-","-","-","VC 100φ",3,"個","-"]
["ダクト器具","排気","ベントキャップ","-","-","-","VC 150φ",5,"個","-"]
["ダクト器具","排気","ベントキャップ","-","-","-","VC 200φ",1,"個","-"]
["ダクト器具","排気","ベントキャップ","-","-","-","VC 250φ",3,"個","-"]
["ダクト器具","排気","レジスター","-","-","-","HS 200×250",2,"個","-"]
["ダクト器具","排気","短管","-","-","-","250×200×150L",2,"個","-"]
["ダクト器具","未設定のダクト","ベントキャップ","-","-","-","VC 100φ",3,"個","-"]
["ダクト器具","未設定のダクト","ベントキャップ","-","-","-","VC 150φ",3,"個","-"]
["ダクト器具","未設定のダクト","ベントキャップ","-","-","-","VC 250φ",2,"個","-"]
["電気","ケーブルラック","ケーブルラック","直線ラック","-","-","300W×70H",50.6,"m","-"]
["電気","ケーブルラック","ケーブルラック","直線ラック","-","-","400W×100H",12.4,"m","-"]
["電気","ケーブルラック","ケーブルラック","外直角L形ベンドラック","-","-","300W×70H",2,"個","-"]
["電気","ケーブルラック","ケーブルラック","外直角L形ベンドラック","-","-","400W×100H",3,"個","-"]
["電気","ケーブルラック","ケーブルラック","T形分岐ラック","-","-","300W×70H-300W×70H",1,"個","-"]
["電気","ケーブルラック","ケーブルラック","上下自在継ぎ金具","-","-","300W×70H",2,"個","-"]
["電気","ケーブルラック","ケーブルラック","上下自在継ぎ金具","-","-","400W×100H",2,"個","-"]
["機器・器具","ファン類","ストレートシロッコファン","ストレートシロッコファン 天吊埋込タイプ 消音形","-","-","BFS-100SUC",2,"台","-"]
["機器・器具","ファン類","ストレートシロッコファン","ストレートシロッコファン 天吊埋込タイプ 消音形","-","-","BFS-120SUC",1,"台","-"]
["機器・器具","ファン類","ストレートシロッコファン","ストレートシロッコファン 天吊埋込タイプ 消音形","-","-","BFS-30SUC",1,"台","-"]
["機器・器具","ファン類","ストレートシロッコファン","ストレートシロッコファン 天吊埋込タイプ 消音形","-","-","BFS-50SUC",2,"台","-"]
["機器・器具","ファン類","ストレートシロッコファン","ストレートシロッコファン 天吊埋込タイプ 消音形","-","-","BFS-65SUC",1,"台","-"]
["機器・器具","ファン類","ラインファン","ラインファン天井吊り形消音","-","-","JFU-550T3",1,"台","-"]
["機器・器具","ファン類","三菱","天井換気扇","-","-","VD-20Z9",1,"台","-"]
["機器・器具","ファン類","全熱交換器","全熱交換器 天井カセット形","-","-","LGH-N15CX",2,"台","-"]
["機器・器具","ファン類","全熱交換器","全熱交換器 天井埋込形","-","-","LGH-N15RX",3,"台","-"]
["機器・器具","ファン類","全熱交換器","全熱交換器 天井埋込形","-","-","LGH-N25RX",3,"台","-"]
["機器・器具","パッケージエアコン","ビル用マルチ","ダブルフローカセット形 ビル用マルチエアコン","-","-","FXYCP36MB",3,"台","-"]
["機器・器具","パッケージエアコン","ビル用マルチ","ラウンドフローカセット形 ビル用マルチエアコン","-","-","FXYFP28MJ",2,"台","-"]
["機器・器具","パッケージエアコン","ビル用マルチ","ラウンドフローカセット形 ビル用マルチエアコン","-","-","FXYFP36MJ",2,"台","-"]
["機器・器具","パッケージエアコン","ビル用マルチ","ラウンドフローカセット形 ビル用マルチエアコン","-","-","FXYFP45MJ",2,"台","-"]
["機器・器具","パッケージエアコン","ビル用マルチ","ラウンドフローカセット形 ビル用マルチエアコン","-","-","FXYFP80MJ",1,"台","-"]
["機器・器具","パッケージエアコン","ビル用マルチ","天井吊形 ビル用マルチエアコン","-","-","SZRH56BAV",1,"台","-"]
["機器・器具","アクセサリー","パブリックアクセサリー","棚付ワンタッチ式紙巻器","-","-","CF-63HST",4,"個","-"]
["機器・器具","消火機器","消火栓･放水口ボックス","屋内消火栓","-","-","750×200×1400",8,"個","-"]
["機器・器具","支持金物","U字金具","Uボルト","-","-","50A",1,"個","-"]
["機器・器具","支持金物","U字金具","Uボルト","-","-","65A",3,"個","-"]
["機器・器具","支持金物","U字金具","Uボルト","-","-","80A",2,"個","-"]
["機器・器具","支持金物","U字金具","Uボルト","-","-","100A",3,"個","-"]
["機器・器具","支持金物","固定金具","立バンド","-","-","20A",1,"個","-"]
["機器・器具","支持金物","固定金具","立バンド","-","-","VP25",11,"個","-"]
["機器・器具","トイレ","小便器","センサー一体形ストール小便器 壁掛タイプ","-","-","U-A51AP",4,"個","-"]
["機器・器具","トイレ","腰掛便器","便器","-","-","C-P25S-AY",4,"個","-"]
["機器・器具","フード","フード","フード","-","-","W-60SAM",2,"個","-"]
["機器・器具","リスト","フォルダ","フォルダ","-","-","EWG-60FTA-Ｑ",1,"個","-"]
["機器・器具","リスト","吸排気グリル","吸排気グリル","-","-","ＰＺ-Ｎ10ＦＧ",6,"個","-"]
["機器・器具","リスト","吸排気グリル","吸排気グリル","-","-","ＰＺ-Ｎ15ＦＧ",6,"個","-"]
["機器・器具","リスト","洗面","SK","-","-","S-202A",1,"個","-"]
["機器・器具","リスト","洗面","洗面","-","-","L259_カウンターL=1800",2,"個","-"]
["機器・器具","リスト","鏡","防錆化粧鏡","-","-","KF-W600H850",4,"個","-"]
["機器・器具","換気扇類","天井扇","天井換気扇","-","-","VD-18ZB10",1,"個","-"]
["機器・器具","換気扇類","天井扇","天井換気扇","-","-","VD-23ZB10",1,"個","-"]
["機器・器具","搬送機器","ウェザーカバー","ウェザーカバー","-","-","W-20SA",1,"個","-"]
["機器・器具","防火区画貫通部材","-","防火区画貫通材","-","-","IRC-125N",3,"個","-"]
["鋼材","山形鋼","50×50×4×4 [3.06Kg/m]","-","-","-",206,1,"本",0.63]
["鋼材","山形鋼","50×50×4×4 [3.06Kg/m]","-","-","-",300,2,"本",1.84]
["鋼材","山形鋼","50×50×4×4 [3.06Kg/m]","-","-","-",353.55,1,"本",1.08]
["鋼材","山形鋼","50×50×4×4 [3.06Kg/m]","-","-","-",1277,1,"本",3.91]
["鋼材","溝形鋼","75×40×5×7 [6.92Kg/m]","-","-","-",350.13,1,"本",2.42]
["鋼材","溝形鋼","75×40×5×7 [6.92Kg/m]","-","-","-",486.13,1,"本",3.36]
["鋼材","平鋼","4×46 [1.444Kg/m]","-","-","-",46,2,"本",0.13]
["スリーブ","1FL","ボイド","-","-","-","80φ×150L",5,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","100φ×120L",4,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","100φ×130L",4,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","100φ×150L",40,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","125φ×120L",1,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","125φ×150L",23,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","150φ×120L",3,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","150φ×130L",3,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","150φ×150L",19,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","175φ×150L",7,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","200φ×120L",2,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","200φ×150L",14,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","250φ×120L",2,"個","-"]
["スリーブ","1FL","ボイド","-","-","-","300φ×150L",1,"個","-"]
["スリーブ","1FL","実管","-","-","-","100φ×150L",10,"個","-"]
["スリーブ","1FL","実管","-","-","-","125φ×120L",1,"個","-"]
["スリーブ","1FL","実管","-","-","-","150φ×150L",11,"個","-"]
["スリーブ","1FL","実管","-","-","-","200φ×150L",2,"個","-"]
["スリーブ","1FL","実管","-","-","-","250φ×150L",7,"個","-"]
["スリーブ","1FL","箱入れ","-","-","-","300W×300H×150L",1,"個","-"]
["スリーブ","1FL","箱入れ","-","-","-","400W×400H×150L",2,"個","-"]
["スリーブ","1FL","箱入れ","-","-","-","400W×400H×171L",1,"個","-"]
["スリーブ","1FL","箱入れ","-","-","-","670W×670H×150L",1,"個","-"]
["スリーブ","1FL","箱入れ","-","-","-","700W×500H×120L",1,"個","-"]
["スリーブ","1FL","箱入れ","-","-","-","700W×500H×150L",1,"個","-"]
["スリーブ","1FL","箱入れ","-","-","-","700W×670H×150L",1,"個","-"]
["スリーブ","2FL","ボイド","-","-","-","80φ×130L",1,"個","-"]
["スリーブ","2FL","ボイド","-","-","-","100φ×130L",1,"個","-"]
["スリーブ","2FL","ボイド","-","-","-","100φ×150L",1,"個","-"]
["kiki","ファン類","天井カセット形","LGH-N15CX","全熱交換器 天井カセット形","-","全熱交換器",2,"台","-"]
["kiki","ファン類","天井吊り形","JFU-550T3","ラインファン天井吊り形消音","-","ラインファン",1,"台","-"]
["kiki","ファン類","天井埋込形","LGH-N15RX","全熱交換器 天井埋込形","-","全熱交換器",3,"台","-"]
["kiki","ファン類","天井埋込形","LGH-N25RX","全熱交換器 天井埋込形","-","全熱交換器",3,"台","-"]
["kiki","ファン類","天井扇(三菱)","VD-20Z9","天井換気扇","-","三菱",1,"台","-"]
["kiki","ファン類","天吊埋込タイプ","BFS-100SUC","ストレートシロッコファン 天吊埋込タイプ 消音形","-","ストレートシロッコファン",2,"台","-"]
["kiki","ファン類","天吊埋込タイプ","BFS-120SUC","ストレートシロッコファン 天吊埋込タイプ 消音形","-","ストレートシロッコファン",1,"台","-"]
["kiki","ファン類","天吊埋込タイプ","BFS-30SUC","ストレートシロッコファン 天吊埋込タイプ 消音形","-","ストレートシロッコファン",1,"台","-"]
["kiki","ファン類","天吊埋込タイプ","BFS-50SUC","ストレートシロッコファン 天吊埋込タイプ 消音形","-","ストレートシロッコファン",2,"台","-"]
["kiki","ファン類","天吊埋込タイプ","BFS-65SUC","ストレートシロッコファン 天吊埋込タイプ 消音形","-","ストレートシロッコファン",1,"台","-"]
["kiki","パッケージエアコン","室内機","FXYCP36MB","ダブルフローカセット形 ビル用マルチエアコン","-","ビル用マルチ",3,"台","-"]
["kiki","パッケージエアコン","室内機","FXYFP28MJ","ラウンドフローカセット形 ビル用マルチエアコン","-","ビル用マルチ",2,"台","-"]
["kiki","パッケージエアコン","室内機","FXYFP36MJ","ラウンドフローカセット形 ビル用マルチエアコン","-","ビル用マルチ",2,"台","-"]
["kiki","パッケージエアコン","室内機","FXYFP45MJ","ラウンドフローカセット形 ビル用マルチエアコン","-","ビル用マルチ",2,"台","-"]
["kiki","パッケージエアコン","室内機","FXYFP80MJ","ラウンドフローカセット形 ビル用マルチエアコン","-","ビル用マルチ",1,"台","-"]
["kiki","パッケージエアコン","室内機","SZRH56BAV","天井吊形 ビル用マルチエアコン","-","ビル用マルチ",1,"台","-"]
["kiki","アクセサリー","棚付ワンタッチ式紙巻器","CF-63HST","棚付ワンタッチ式紙巻器","-","パブリックアクセサリー",4,"個","-"]
["kiki","トイレ","センサー一体形","U-A51AP","センサー一体形ストール小便器 壁掛タイプ","-","小便器",4,"個","-"]

{"sheet":"▼拾い集計","index":3,"n_rows":539,"n_cols":6,"rows_kept":539,"cut":false,"hidden":false,"merged":[]}
[null,"　拾　い　集　計　表　",null,null,null,"2016年09月02日"]
[null,"【隊庁舎】_1F設備_0831"]
[null,"名　称","規　格","数　量","単　位","備　考"]
[null,"配管","",null,""]
[null,"冷媒","",null,""]
[null,"冷媒用銅管(2管式)","12.7φ×6.4φ",56678,"mm"]
[null,"","15.9φ×9.5φ",16744,"mm"]
[null,"","19.1φ×9.5φ",7018,"mm"]
[null,"","34.9φ×9.5φ",19337,"mm"]
[null,"ドレン(空調)","",null,""]
[null,"配管用炭素鋼鋼管(白)","20A",313,"mm"]
[null,"","25A",29993,"mm"]
[null,"","32A",49087,"mm"]
[null,"","40A",42983,"mm"]
[null,"","50A",117,"mm"]
[null,"給水","",null,""]
[null,"水道用硬質塩化ビニルライニング鋼管(屋内外用)","15A",183,"mm"]
[null,"","20A",47701,"mm"]
[null,"","25A",13789,"mm"]
[null,"","32A",5860,"mm"]
[null,"","40A",1641,"mm"]
[null,"","50A",10643,"mm"]
[null,"","65A",1950,"mm"]
[null,"給湯(往)","",null,""]
[null,"一般配管用ステンレス鋼管","20Su",26174,"mm"]
[null,"","25Su",51050,"mm"]
[null,"給湯(還)","",null,""]
[null,"一般配管用ステンレス鋼管","20Su",44116,"mm"]
[null,"","25Su",700,"mm"]
[null,"汚水","",null,""]
[null,"排水用硬質塩化ビニルライニング鋼管","40A",20497,"mm"]
[null,"","50A",39055,"mm"]
[null,"","65A",4675,"mm"]
[null,"","80A",6419,"mm"]
[null,"","100A",44146,"mm"]
[null,"硬質塩化ビニル管(VP)","50A",118,"mm"]
[null,"通気","",null,""]
[null,"排水用硬質塩化ビニルライニング鋼管","65A",6633,"mm"]
[null,"","80A",11131,"mm"]
[null,"配管用炭素鋼鋼管(白)","80A",21424,"mm"]
[null,"屋内消火栓","",null,""]
[null,"配管用炭素鋼鋼管(白)","40A",9536,"mm"]
[null,"","50A",4493,"mm"]
[null,"","65A",39444,"mm"]
[null,"","",null,""]
[null,"継手","",null,""]
[null,"冷媒","",null,""]
[null,"セパレータ","15.9φ(9.5φ)×12.7φ(6.4φ)×12.7φ(6.4φ)",1,"個"]
[null,"","15.9φ(9.5φ)×15.9φ(9.5φ)×12.7φ(6.4φ)",1,"個"]
[null,"","19.1φ(9.5φ)×15.9φ(9.5φ)×12.7φ(6.4φ)",1,"個"]
[null,"","19.1φ(9.5φ)×19.1φ(9.5φ)×12.7φ(6.4φ)",1,"個"]
[null,"","34.9φ(9.5φ)×12.7φ(6.4φ)×12.7φ(6.4φ)",1,"個"]
[null,"","34.9φ(9.5φ)×34.9φ(9.5φ)×12.7φ(6.4φ)",2,"個"]
[null,"ドレン(空調)","",null,""]
[null,"ドレネジ継手","",null,""]
[null,"L","40",3,"個"]
[null,"","50×40",1,"個"]
[null,"P","32",1,"個"]
[null,"S","40×32",1,"個"]
[null,"","50×32",1,"個"]
[null,"","50×40",1,"個"]
[null,"ST","32",13,"個"]
[null,"","40×32",1,"個"]
[null,"TY","40",3,"個"]
[null,"","40×32",3,"個"]
[null,"YL","32",9,"個"]
[null,"","40",3,"個"]
[null,"鋼管継手（白）","",null,""]
[null,"L","25",29,"個"]
[null,"P","25",15,"個"]
[null,"","32",7,"個"]
[null,"","40",3,"個"]
[null,"S","25",2,"個"]
[null,"","25×20",1,"個"]
[null,"","32×25",10,"個"]
[null,"T","25",14,"個"]
[null,"YL","25",4,"個"]
[null,"給水","",null,""]
[null,"メーター接続金具","",null,""]
[null,"ガス管用U","25",3,"個"]
[null,"屋内用管端防食継手","",null,""]
[null,"L","20",41,"個"]
[null,"","25",11,"個"]
[null,"","32",2,"個"]
[null,"","40",1,"個"]
[null,"","50",5,"個"]
[null,"","20×15",1,"個"]
[null,"S","20×15",5,"個"]
[null,"","25×20",4,"個"]
[null,"","32×20",1,"個"]
[null,"","32×25",1,"個"]
[null,"","40×32",1,"個"]
[null,"","50×32",1,"個"]
[null,"","65×50",1,"個"]
[null,"T","20",2,"個"]
[null,"","25",1,"個"]
[null,"","50",1,"個"]
[null,"","25×20",7,"個"]
[null,"","32×20",4,"個"]
[null,"","32×25",4,"個"]
[null,"","40×25",2,"個"]
[null,"","50×40",1,"個"]
[null,"","65×50",1,"個"]
[null,"YL","50",1,"個"]
[null,"給水栓L","20",1,"個"]
[null,"鋳鉄製フランジ","",null,""]
[null,"F10K","65",2,"個"]
[null,"給湯(往)","",null,""]
[null,"BKジョイント","",null,""]
[null,"L","20",16,"個"]
[null,"","25",17,"個"]
[null,"S","25×20",4,"個"]
[null,"T","20",4,"個"]
[null,"","25",5,"個"]
[null,"","25×20",4,"個"]
[null,"YL","25",2,"個"]
[null,"水栓S","20×15",1,"個"]
[null,"雄アダプタ付S","20×20",1,"個"]
[null,"","25×25",4,"個"]
[null,"給湯(還)","",null,""]
[null,"BKジョイント","",null,""]
[null,"L","20",21,"個"]
[null,"","25",1,"個"]
[null,"S","20",1,"個"]
[null,"T","20",3,"個"]
[null,"","25×20",1,"個"]
[null,"雄アダプタ付S","20×20",4,"個"]
[null,"モルコジョイント","",null,""]
[null,"S","25×20",1,"個"]
[null,"汚水","",null,""]
[null,"MDジョイント","",null,""]
[null,"LL","40",12,"個"]
[null,"","50",26,"個"]
[null,"","65",4,"個"]
[null,"","80",4,"個"]
[null,"","100",8,"個"]
[null,"S","100",1,"個"]
[null,"ST","100×80",3,"個"]
[null,"TY","50",2,"個"]
[null,"","100",5,"個"]
[null,"","100×40",4,"個"]
[null,"","100×50",8,"個"]
[null,"","100×65",3,"個"]
[null,"","100×80",4,"個"]
[null,"Y","100",2,"個"]
[null,"","100×40",1,"個"]
[null,"","100×50",3,"個"]
[null,"YL","40",6,"個"]
[null,"","50",2,"個"]
[null,"","65",1,"個"]
[null,"","80",5,"個"]
[null,"","100",8,"個"]
[null,"パッキンセット","40",41,"個"]
[null,"","50",73,"個"]
[null,"","65",13,"個"]
[null,"","80",25,"個"]
[null,"","100",109,"個"]
[null,"満水試験用COS","100",2,"個"]
[null,"通気","",null,""]
[null,"MDジョイント","",null,""]
[null,"LL","65",2,"個"]
[null,"","80",13,"個"]
[null,"ST","80×65",2,"個"]
[null,"Y","80",1,"個"]
[null,"","80×65",1,"個"]
[null,"YL","65",3,"個"]
[null,"","80",4,"個"]
[null,"パッキンセット","65",13,"個"]
[null,"","80",43,"個"]
[null,"屋内消火栓","",null,""]
[null,"鋳鉄製フランジ","",null,""]
[null,"F10K","65",1,"個"]
[null,"鋼管継手（白）","",null,""]
[null,"L","40",10,"個"]
[null,"","65",8,"個"]
[null,"","50×40",1,"個"]
[null,"S","50",1,"個"]
[null,"","50×40",2,"個"]
[null,"T","65",1,"個"]
[null,"","50×40×40",1,"個"]
[null,"","50×40×65",1,"個"]
[null,"","50×50×65",1,"個"]
[null,"","",null,""]
[null,"弁類･特殊継手","",null,""]
[null,"給水","",null,""]
[null,"青銅製仕切弁(ねじ込み形)JIS10K","50",2,"個"]
[null,"給湯(往)","",null,""]
[null,"自動空気抜き弁(ねじ込み形)","20",1,"個"]
[null,"青銅製仕切弁(ねじ込み形)JIS10K","20",1,"個"]
[null,"","25",2,"個"]
[null,"給湯(還)","",null,""]
[null,"青銅製仕切弁(ねじ込み形)JIS10K","20",2,"個"]
[null,"汚水","",null,""]
[null,"COA 掃除口(ねじ込み形)","50",2,"個"]
[null,"","100",1,"個"]
[null,"COB 掃除口(防水用)","100",6,"個"]
[null,"T3B 床排水トラップ(Pトラップ式)防水用","65",2,"個"]
[null,"未設定の配管","",null,""]
[null,"サクションカバー(相フランジ形)","65",1,"個"]
[null,"","",null,""]
[null,"ダクト","",null,""]
[null,"給気","",null,""]
[null,"主管","",null,""]
[null,"アルミフレキ 100φ","400L",1,"本"]
[null,"","440L",1,"本"]
[null,"","550L",1,"本"]
[null,"","650L",1,"本"]
[null,"","760L",1,"本"]
[null,"アルミフレキ 150φ","550L",1,"本"]
[null,"ニューホープ 100φ","410L",1,"本"]
[null,"スパイラルダクト","",null,""]
[null,"主管","",null,""]
[null,"亜鉛鉄板","100φ",19600.208999999999,"mm",0.5]
[null,"","150φ",11400.626,"mm",0.5]
[null,"外気","",null,""]
[null,"アングルフランジダクト","",null,""]
[null,"300×200","",null,""]
[null,"亜鉛鉄板","0.5mm",0.66,"㎡"]
[null,"共板フランジダクト","",null,""]
[null,"300×200","",null,""]
[null,"亜鉛鉄板","0.5mm",5.8159999999999998,"㎡"]
[null,"主管","",null,""]
[null,"ニューホープ 100φ","1670L",1,"本"]
[null,"","3470L",1,"本"]
[null,"","3570L",1,"本"]
[null,"ニューホープ 150φ","2270L",1,"本"]
[null,"","2320L",1,"本"]
[null,"","2460L",1,"本"]
[null,"スパイラルダクト","",null,""]
[null,"主管","",null,""]
[null,"亜鉛鉄板","100φ",8561.1290000000008,"mm",0.5]
[null,"","150φ",1729.2639999999999,"mm",0.5]
[null,"","200φ",3532.7640000000001,"mm",0.5]
[null,"","250φ",14364.291999999999,"mm",0.5]
[null,"排気","",null,""]
[null,"共板フランジダクト","",null,""]
[null,"600×400","",null,""]
[null,"亜鉛鉄板","0.6mm",15.090999999999999,"㎡"]
[null,"700×670","",null,""]
[null,"亜鉛鉄板","0.6mm",1.548,"㎡"]
[null,"円形フランジダクト","",null,""]
[null,"主管","",null,""]
[null,"亜鉛鉄板","750φ",375,"mm",0.8]
[null,"主管","",null,""]
[null,"アルミフレキ 100φ","400L",1,"本"]
[null,"","480L",1,"本"]
[null,"","500L",1,"本"]
[null,"","560L",1,"本"]
[null,"","790L",1,"本"]
[null,"アルミフレキ 150φ","550L",1,"本"]
[null,"アルミフレキ 250φ","430L",1,"本"]
[null,"","840L",1,"本"]
[null,"ニューホープ 100φ","400L",1,"本"]
[null,"","1660L",1,"本"]
[null,"","1940L",1,"本"]
[null,"","2150L",1,"本"]
[null,"ニューホープ 150φ","2130L",1,"本"]
[null,"","2350L",1,"本"]
[null,"","2620L",1,"本"]
[null,"スパイラルダクト","",null,""]
[null,"主管","",null,""]
[null,"亜鉛鉄板","100φ",32937.086000000003,"mm",0.5]
[null,"","150φ",37720.432000000001,"mm",0.5]
[null,"","200φ",8883.7810000000009,"mm",0.5]
[null,"","250φ",14887.339,"mm",0.5]
[null,"未設定のダクト","",null,""]
[null,"スパイラルダクト","",null,""]
[null,"主管","",null,""]
[null,"亜鉛鉄板","150φ",50,"mm",0.5]
[null,"","200φ",150.94300000000001,"mm",0.5]
[null,"","250φ",50,"mm",0.5]
[null,"","",null,""]
[null,"ダクト継手","",null,""]
[null,"給気","",null,""]
[null,"スパイラルダクト継手(亜鉛鉄板)","",null,""]
[null,"L","",null,""]
[null,"100","",7,"個",0.5]
[null,"150","",6,"個",0.5]
[null,"YL","",null,""]
[null,"100","",4,"個",0.5]
[null,"150","",6,"個",0.5]
[null,"差込継手","",null,""]
[null,"100","",5,"個",0.5]
[null,"100","",2,"個"]
[null,"150","",1,"個",0.5]
[null,"外気","",null,""]
[null,"スパイラルダクト継手(亜鉛鉄板)","",null,""]
[null,"L","",null,""]
[null,"100","",3,"個",0.5]
[null,"YL","",null,""]
[null,"100","",2,"個",0.5]
[null,"150","",2,"個",0.5]
[null,"200","",2,"個",0.5]
[null,"250","",6,"個",0.5]
[null,"差込継手","",null,""]
[null,"100","",1,"個"]
[null,"100","",3,"個",0.5]
[null,"150","",3,"個",0.5]
[null,"排気","",null,""]
[null,"スパイラルダクト継手(亜鉛鉄板)","",null,""]
[null,"L","",null,""]
[null,"100","",8,"個",0.5]
[null,"150","",13,"個",0.5]
[null,"200","",3,"個",0.5]
[null,"S","",null,""]
[null,"250×200","",1,"個"]
[null,"250×200","",6,"個",0.5]
[null,"T","",null,""]
[null,"250×200","",1,"個",0.5]
[null,"YL","",null,""]
[null,"100","",10,"個",0.5]
[null,"150","",18,"個",0.5]
[null,"200","",2,"個",0.5]
[null,"250","",11,"個",0.5]
[null,"差込継手","",null,""]
[null,"100","",1,"個"]
[null,"100","",11,"個",0.5]
[null,"150","",7,"個",0.5]
[null,"250","",3,"個",0.5]
[null,"円形ダクト継手(亜鉛鉄板)","",null,""]
[null,"レデューサー","",null,""]
[null,"500×750","",1,"個",0.8]
[null,"","",null,""]
[null,"ダクト器具","",null,""]
[null,"給気","",null,""]
[null,"FD","100φ×200L",1,"個"]
[null,"","100φ×300L",1,"個"]
[null,"キャンバス継手","100φ×200L",1,"個"]
[null,"","150φ×200L",4,"個"]
[null,"外気","",null,""]
[null,"ボックス(内貼り 25mm)","550×550×400H",2,"個"]
[null,"FD","100φ×300L",1,"個"]
[null,"","300×200×200L",1,"個"]
[null,"キャンバス継手","100φ×200L",1,"個"]
[null,"","200φ×200L",1,"個"]
[null,"ベントキャップ","VC 100φ",4,"個"]
[null,"","VC 150φ",3,"個"]
[null,"","VC 200φ",1,"個"]
[null,"","VC 250φ",2,"個"]
[null,"レジスター","VHS 350×350",2,"個"]
[null,"短管","350×350×150L",2,"個"]
[null,"排気","",null,""]
[null,"ボックス(内貼り 25mm)","400×450×400H",2,"個"]
[null,"FD","100φ×200L",1,"個"]
[null,"","100φ×300L",2,"個"]
[null,"","150φ×200L",1,"個"]
[null,"","150φ×300L",2,"個"]
[null,"","200φ×300L",1,"個"]
[null,"","250φ×200L",1,"個"]
[null,"キャンバス継手","100φ×200L",2,"個"]
[null,"","150φ×200L",8,"個"]
[null,"","200φ×200L",3,"個"]
[null,"","250φ×200L",1,"個"]
[null,"","600×400(500φ)×362L",1,"個"]
[null,"ベントキャップ","VC 100φ",3,"個"]
[null,"","VC 150φ",5,"個"]
[null,"","VC 200φ",1,"個"]
[null,"","VC 250φ",3,"個"]
[null,"レジスター","HS 200×250",2,"個"]
[null,"短管","250×200×150L",2,"個"]
[null,"未設定のダクト","",null,""]
[null,"ベントキャップ","VC 100φ",3,"個"]
[null,"","VC 150φ",3,"個"]
[null,"","VC 250φ",2,"個"]
[null,"","",null,""]
[null,"電気","",null,""]
[null,"ケーブルラック","",null,""]
[null,"ケーブルラック","",null,""]
[null,"直線ラック","300W×70H",50.6,"m"]
[null,"","400W×100H",12.4,"m"]
[null,"外直角L形ベンドラック","300W×70H",2,"個"]
[null,"","400W×100H",3,"個"]
[null,"T形分岐ラック","300W×70H-300W×70H",1,"個"]
[null,"上下自在継ぎ金具","300W×70H",2,"個"]
[null,"","400W×100H",2,"個"]
[null,"","",null,""]
[null,"機器・器具","",null,""]
[null,"ファン類","",null,""]
[null,"ストレートシロッコファン","",null,""]
[null,"ストレートシロッコファン 天吊埋込タイプ 消音形","BFS-100SUC",2,"台"]
[null,"","BFS-120SUC",1,"台"]
[null,"","BFS-30SUC",1,"台"]
[null,"","BFS-50SUC",2,"台"]
[null,"","BFS-65SUC",1,"台"]
[null,"ラインファン","",null,""]
[null,"ラインファン天井吊り形消音","JFU-550T3",1,"台"]
[null,"三菱","",null,""]
[null,"天井換気扇","VD-20Z9",1,"台"]
[null,"全熱交換器","",null,""]
[null,"全熱交換器 天井カセット形","LGH-N15CX",2,"台"]
[null,"全熱交換器 天井埋込形","LGH-N15RX",3,"台"]
[null,"","LGH-N25RX",3,"台"]
[null,"パッケージエアコン","",null,""]
[null,"ビル用マルチ","",null,""]
[null,"ダブルフローカセット形 ビル用マルチエアコン","FXYCP36MB",3,"台"]
[null,"ラウンドフローカセット形 ビル用マルチエアコン","FXYFP28MJ",2,"台"]
[null,"","FXYFP36MJ",2,"台"]
[null,"","FXYFP45MJ",2,"台"]
[null,"","FXYFP80MJ",1,"台"]
[null,"天井吊形 ビル用マルチエアコン","SZRH56BAV",1,"台"]
[null,"アクセサリー","",null,""]
[null,"パブリックアクセサリー","",null,""]
[null,"棚付ワンタッチ式紙巻器","CF-63HST",4,"個"]
[null,"消火機器","",null,""]
[null,"消火栓･放水口ボックス","",null,""]
[null,"屋内消火栓","750×200×1400",8,"個"]
[null,"支持金物","",null,""]
[null,"U字金具","",null,""]
[null,"Uボルト","50A",1,"個"]
[null,"","65A",3,"個"]
[null,"","80A",2,"個"]
[null,"","100A",3,"個"]
[null,"固定金具","",null,""]
[null,"立バンド","20A",1,"個"]
[null,"","VP25",11,"個"]
[null,"トイレ","",null,""]
[null,"小便器","",null,""]
[null,"センサー一体形ストール小便器 壁掛タイプ","U-A51AP",4,"個"]
[null,"腰掛便器","",null,""]
[null,"便器","C-P25S-AY",4,"個"]
[null,"フード","",null,""]
[null,"フード","",null,""]
[null,"フード","W-60SAM",2,"個"]
[null,"リスト","",null,""]
[null,"フォルダ","",null,""]
[null,"フォルダ","EWG-60FTA-Ｑ",1,"個"]
[null,"吸排気グリル","",null,""]
[null,"吸排気グリル","ＰＺ-Ｎ10ＦＧ",6,"個"]
[null,"","ＰＺ-Ｎ15ＦＧ",6,"個"]
[null,"洗面","",null,""]
[null,"SK","S-202A",1,"個"]
[null,"洗面","L259_カウンターL=1800",2,"個"]
[null,"鏡","",null,""]
[null,"防錆化粧鏡","KF-W600H850",4,"個"]
[null,"換気扇類","",null,""]
[null,"天井扇","",null,""]
[null,"天井換気扇","VD-18ZB10",1,"個"]
[null,"","VD-23ZB10",1,"個"]
[null,"搬送機器","",null,""]
[null,"ウェザーカバー","",null,""]
[null,"ウェザーカバー","W-20SA",1,"個"]
[null,"防火区画貫通部材","",null,""]
[null,"","",null,""]
[null,"防火区画貫通材","IRC-125N",3,"個"]
[null,"","",null,""]
[null,"鋼材","",null,""]
[null,"山形鋼","",null,""]
[null,"50×50×4×4 [3.06Kg/m]",206,1,"本",0.63]
[null,"",300,2,"本",1.84]
[null,"",353.55,1,"本",1.08]
[null,"",1277,1,"本",3.91]
[null,"溝形鋼","",null,""]
[null,"75×40×5×7 [6.92Kg/m]",350.13,1,"本",2.42]
[null,"",486.13,1,"本",3.36]
[null,"平鋼","",null,""]
[null,"4×46 [1.444Kg/m]",46,2,"本",0.13]
[null,"","",null,""]
[null,"スリーブ","",null,""]
[null,"1FL","",null,""]
[null,"ボイド","80φ×150L",5,"個"]
[null,"","100φ×120L",4,"個"]
[null,"","100φ×130L",4,"個"]
[null,"","100φ×150L",40,"個"]
[null,"","125φ×120L",1,"個"]
[null,"","125φ×150L",23,"個"]
[null,"","150φ×120L",3,"個"]
[null,"","150φ×130L",3,"個"]
[null,"","150φ×150L",19,"個"]
[null,"","175φ×150L",7,"個"]
[null,"","200φ×120L",2,"個"]
[null,"","200φ×150L",14,"個"]
[null,"","250φ×120L",2,"個"]
[null,"","300φ×150L",1,"個"]
[null,"実管","100φ×150L",10,"個"]
[null,"","125φ×120L",1,"個"]
[null,"","150φ×150L",11,"個"]
[null,"","200φ×150L",2,"個"]
[null,"","250φ×150L",7,"個"]
[null,"箱入れ","300W×300H×150L",1,"個"]
[null,"","400W×400H×150L",2,"個"]
[null,"","400W×400H×171L",1,"個"]
[null,"","670W×670H×150L",1,"個"]
[null,"","700W×500H×120L",1,"個"]
[null,"","700W×500H×150L",1,"個"]
[null,"","700W×670H×150L",1,"個"]
[null,"2FL","",null,""]
[null,"ボイド","80φ×130L",1,"個"]
[null,"","100φ×130L",1,"個"]
[null,"","100φ×150L",1,"個"]
[null,"","",null,""]
[null,"kiki","",null,""]
[null,"ファン類","",null,""]
[null,"天井カセット形","",null,""]
[null,"LGH-N15CX","",null,""]
[null,"全熱交換器 天井カセット形","全熱交換器",2,"台"]
[null,"天井吊り形","",null,""]
[null,"JFU-550T3","",null,""]
[null,"ラインファン天井吊り形消音","ラインファン",1,"台"]
[null,"天井埋込形","",null,""]
[null,"LGH-N15RX","",null,""]
[null,"全熱交換器 天井埋込形","全熱交換器",3,"台"]
[null,"LGH-N25RX","",null,""]
[null,"全熱交換器 天井埋込形","全熱交換器",3,"台"]
[null,"天井扇(三菱)","",null,""]
[null,"VD-20Z9","",null,""]
[null,"天井換気扇","三菱",1,"台"]
[null,"天吊埋込タイプ","",null,""]
[null,"BFS-100SUC","",null,""]
[null,"ストレートシロッコファン 天吊埋込タイプ 消音形","ストレートシロッコファン",2,"台"]
[null,"BFS-120SUC","",null,""]
[null,"ストレートシロッコファン 天吊埋込タイプ 消音形","ストレートシロッコファン",1,"台"]
[null,"BFS-30SUC","",null,""]
[null,"ストレートシロッコファン 天吊埋込タイプ 消音形","ストレートシロッコファン",1,"台"]
[null,"BFS-50SUC","",null,""]
[null,"ストレートシロッコファン 天吊埋込タイプ 消音形","ストレートシロッコファン",2,"台"]
[null,"BFS-65SUC","",null,""]
[null,"ストレートシロッコファン 天吊埋込タイプ 消音形","ストレートシロッコファン",1,"台"]
[null,"パッケージエアコン","",null,""]
[null,"室内機","",null,""]
[null,"FXYCP36MB","",null,""]
[null,"ダブルフローカセット形 ビル用マルチエアコン","ビル用マルチ",3,"台"]
[null,"FXYFP28MJ","",null,""]
[null,"ラウンドフローカセット形 ビル用マルチエアコン","ビル用マルチ",2,"台"]
[null,"FXYFP36MJ","",null,""]
[null,"ラウンドフローカセット形 ビル用マルチエアコン","ビル用マルチ",2,"台"]
[null,"FXYFP45MJ","",null,""]
[null,"ラウンドフローカセット形 ビル用マルチエアコン","ビル用マルチ",2,"台"]
[null,"FXYFP80MJ","",null,""]
[null,"ラウンドフローカセット形 ビル用マルチエアコン","ビル用マルチ",1,"台"]
[null,"SZRH56BAV","",null,""]
[null,"天井吊形 ビル用マルチエアコン","ビル用マルチ",1,"台"]
[null,"アクセサリー","",null,""]
[null,"棚付ワンタッチ式紙巻器","",null,""]
[null,"CF-63HST","",null,""]
[null,"棚付ワンタッチ式紙巻器","パブリックアクセサリー",4,"個"]
[null,"トイレ","",null,""]
[null,"センサー一体形","",null,""]
[null,"U-A51AP","",null,""]
[null,"センサー一体形ストール小便器 壁掛タイプ","小便器",4,"個"]